Current Measurements of Sensor PCB

@5V

Startup - 13.6mA

Sensor Reading - 16.1mA

Tx active - 15.2mA

Sleep - 4.7mA